{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["温度ヒューズ"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"温度ヒューズ","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[[5,2,5,6],[5,0,5,1],[7,0,8,0],[9,0,12,0],[13,0,25,0],[3,0,3,1],[4,0,4,1],[32,0,33,0],[34,0,36,0],[37,0,39,0],[26,0,27,0],[28,0,31,0]]}
[]
["電気用品の区分","温度ヒューズ"]
["電気用品名","温度ヒューズ"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格電流","（１）　５Ａ以下のもの"]
[null,"（２）　５Ａを超え１５Ａ以下のもの"]
[null,"（３）　１５Ａを超え３０Ａ以下のもの"]
[null,"（４）　３０Ａを超えるもの"]
["公称動作温度","（１）　８０℃以下のもの"]
[null,"（２）　８０℃を超え１００℃以下のもの"]
[null,"（３）　１００℃を超え１２０℃以下のもの"]
[null,"（４）　１２０℃を超え１４０℃以下のもの"]
[null,"（５）　１４０℃を超え１６０℃以下のもの"]
[null,"（６）　１６０℃を超え１８０℃以下のもの"]
[null,"（７）　１８０℃を超え２００℃以下のもの"]
[null,"（８）　２００℃を超え２２０℃以下のもの"]
[null,"（９）　２２０℃を超え２４０℃以下のも"]
[null,"（１０）　２４０℃を超え２６０℃以下のもの"]
[null,"（１１）　２６０℃を超え２８０℃以下のもの"]
[null,"（１２）　２８０℃を超え３００℃以下のもの"]
[null,"（１３）　３００℃を超えるもの"]
["可溶体への通電","（１）　あるもの"]
[null,"（２）　ないもの"]
["可溶体の主材料","（１）　すず、鉛及びビスマスの合金のもの"]
[null,"（２）　すず、鉛及びビスマスの合金以外の合金のもの"]
[null,"（３）　合成樹脂又は有機化合物のもの"]
[null,"（４）　その他のもの"]
["容器","（１）　あるもの"]
[null,"（２）　ないもの"]
["端子","（１）　つめ形（丸形を含む。）のもの"]
[null,"（２）　線付きのもの"]
[null,"（３）　その他のもの"]
["可溶体の形状","（１）　板状のもの"]
[null,"（２）　塊状のもの"]
[null,"（３）　その他もの"]