{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["13インデックス","反発始動誘導電動機","分相始動誘導電動機","コンデンサー始動誘導電動機","コンデンサー誘導電動機","整流子電動機","くま取りコイル誘導電動機","その他の単相電動機","かご形三相誘導電動機"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"13インデックス","index":0,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["小形交流電動機"]
[]
["特定電気用品以外の電気用品"]
[null,"反発始動誘導電動機"]
[null,"分相始動誘導電動機"]
[null,"コンデンサー始動誘導電動機"]
[null,"コンデンサー誘導電動機"]
[null,"整流子電動機"]
[null,"くま取りコイル誘導電動機"]
[null,"その他の単相電動機"]
[null,"かご形三相誘導電動機"]

{"sheet":"反発始動誘導電動機","index":1,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","反発始動誘導電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"分相始動誘導電動機","index":2,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","分相始動誘導電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"コンデンサー始動誘導電動機","index":3,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","コンデンサー始動誘導電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"コンデンサー誘導電動機","index":4,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","コンデンサー誘導電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"整流子電動機","index":5,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","整流子電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"くま取りコイル誘導電動機","index":6,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","くま取りコイル誘導電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"その他の単相電動機","index":7,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[21,0,23,0],[24,0,26,0],[27,0,28,0],[29,0,30,0],[4,0,4,1],[4,2,4,6],[6,0,7,0],[8,0,9,0],[10,0,15,0],[16,0,17,0],[18,0,20,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","その他の単相電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格電圧","（１）　１２５Ｖ以下のもの"]
[null,"（２）　１２５Ｖを超えるもの"]
["定格入力（定格出力が５０Ｗ以下のものの場合に限る。）","（１）　６０Ｗ以下のもの"]
[null,"（２）　６０Ｗを超えるもの"]
["定格出力（定格出力が５０Ｗを超えるものの場合に限る。）","（１）　８０Ｗ以下のもの"]
[null,"（２）　８０Ｗを超え１２５Ｗ以下のもの"]
[null,"（３）　１２５Ｗを超え２００Ｗ以下のもの"]
[null,"（４）　２００Ｗを超え３００Ｗ以下のもの"]
[null,"（５）　３００Ｗを超え４００Ｗ以下のもの"]
[null,"（６）　４００Ｗを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["定格時間","（１）　短時間定格のもの"]
[null,"（２）　反復定格のもの（ミシン用電動機の場合を除く。）"]
[null,"（３）　連続定格のもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["進相用コンデンサー","（１）　あるもの"]
[null,"（２）　ないもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]

{"sheet":"かご形三相誘導電動機","index":8,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[4,2,4,6],[4,0,4,1],[22,0,23,0],[6,0,11,0],[12,0,13,0],[14,0,16,0],[17,0,18,0],[19,0,21,0]]}
["電気用品の区分","小形交流電動機"]
["電気用品名","かご形三相誘導電動機"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["定格出力","（１）　２００Ｗ以下のもの"]
[null,"（２）　２００Ｗを超え４００Ｗ以下のもの"]
[null,"（３）　４００Ｗを超え７００Ｗ以下のもの"]
[null,"（４）　７００Ｗを超え１．２ｋＷ以下のもの"]
[null,"（５）　１．２ｋＷを超え１．８ｋＷ以下のもの"]
[null,"（６）　１．８ｋＷを超えるもの"]
["定格周波数","（１）　５０Ｈｚのもの"]
[null,"（２）　６０Ｈｚのもの"]
["極","（１）　２極のもの"]
[null,"（２）　４極のもの"]
[null,"（３）　６極以上のもの"]
["外被","（１）　全閉型のもの"]
[null,"（２）　開放型のもの"]
["巻線の絶縁の種類","（１）　Ａ種のもの"]
[null,"（２）　Ｅ種のもの"]
[null,"（３）　その他のもの"]
["過負荷保護装置","（１）　あるもの"]
[null,"（２）　ないもの"]