{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["リチウムイオン蓄電池"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"リチウムイオン蓄電池","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[[5,2,5,6],[5,0,5,1],[7,0,9,0],[10,0,11,0],[12,0,13,0],[3,0,3,1],[4,0,4,1],[18,0,19,0],[20,0,22,0],[23,0,24,0],[14,0,15,0],[16,0,17,0]]}
[]
["電気用品の区分","リチウムイオン蓄電池"]
["電気用品名","リチウムイオン蓄電池"]
["届出の内容（新規届出／追加／削除の別）"]
["製品名・型番等（メモ欄）"]
["型式の区分",null,"整理番号等"]
["要素","区分","①","②","③","④","⑤"]
["単電池の形状","（１）　円筒形のもの"]
[null,"（２）　角形のもの"]
[null,"（３）　その他のもの"]
["単電池の電解質の種類","（１）　液体状のもの"]
[null,"（２）　その他のもの"]
["単電池の上限充電電圧","（１）　４．２５Ｖ以下のもの"]
[null,"（２）　４．２５Ｖを超えるもの"]
["組電池の質量","（１）　７ｋｇ以下のもの"]
[null,"（２）　７ｋｇを超えるもの"]
["電池ブロックの個数","（１）　１個のもの"]
[null,"（２）　２個以上のもの"]
["過充電の保護機能","（１）　組電池で制御するもの"]
[null,"（２）　組電池搭載機器又は充電器で制御するもの"]
["用途","（１）　携帯機器用のもの"]
[null,"（２）　卓上機器用のもの"]
[null,"（３）　その他のもの"]
["組電池の種類","（１）　はんだ付けその他の接合方法により、容易に取り外すことができない状態で機械器具に固定して用いられるものその他の特殊な構造のもの"]
[null,"（２）　その他のもの"]